Helical Coil Instruction
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NTW-screw type (torsert) nib tap uses helical coil for sizes M14 or larger. The shanks have pre-set helical coil when delivered. When helical coil breaks, the replacement procedures are as follows:


1. At first, remove the broken helical coil in the shank by using a broken coil extractor.
2. Then mount a new helical coil by a coil layer (the bent portion of the coil is placed in the gap at the top of the layer at this stage), screw to an extent where it cannot be turned further. 
3. When the helical coil has been screwed down to an extent where it cannot be turned any further, the layer can be pulled out easily. The helical coil is now properly set in the shank. For next you can mount a new nib tap and start to use again. 
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