Maintenance of Streicher TC-16 Tapping Machine

                                                        Daily Maintenance
.  Check the oil level for the tapping oil on the oil-level gauge on the front of the machine and if necessary, replenish oil.
.  Check the magnetic drum to see if swarf or nuts have become jammed and if so, remove them.
.  Get rid of any swarf in the working area.
.  De-grease the swarf, clean it and dispose of it in an eco-friendly way, in   accordance with regulations.
.  Check the machine for obvious damage and defects.  
.  Check Air Pressure and make sure no moisture in air lines.
.  Cycle Carriage unit a few times to make sure jaws up and close properly.

Weekly Maintenance
.  Check the oil level in the advance device housing and, if necessary, replenish with tapping oil until the disk cams plunge approximately 1 inch into the oil with their highest points.

Monthly Maintenance
.  Clean all the polished surfaces of the machine with a cleaning cloth, if they are heavily soiled, use a domestic cleaner as well.
.  Blow out all the filters in the doors of the control cabinet, or, if they are heavily soiled, replace them (refer to the manufactures instruction manual for this).
.  Grease (3) nipples behind ejection head door with one stroke of hand lubrication press with standard bearing grease.

 
Six-Months Maintenance
.  Clean the entire tapping oil reservoir.  To this end, remove the magnetic roller and pump off the oil.  Dispose of the old oil and sludge properly and in an eco-friendly way.
.  Clean the working area, and all surfaces sliding on one another.  Remove even the smallest slivers.
.  Check the machines electrical equipment.  Defects, such as loose connections, singed cables or oily operating means must be eliminated immediately.  
 



